<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>ICSP Programming Header</text>
<text>+3.3V</text>
<text>GND</text>
<text>MCLR</text>
<text>DATA</text>
<text>CLOCK</text>
<text>I/O header</text>
<text>PWR</text>
<text>MODE</text>
<text>VREG</text>
<text>BPv3.9</text>
<text>PWR</text>
<text>MODE</text>
<text>VREG</text>
<text>USB</text>
<text>USB</text>
<text>5V</text>
<text>GND</text>
<text>ADC</text>
<text>CS</text>
<text>CLK</text>
<text>3V3</text>
<text>VPU</text>
<text>AUX</text>
<text>MISO</text>
<text>MOSI</text>
<text>Seeed Studio</text>
<text>www.seeedstudio.com</text>
<text>I+S 2018</text>
<text>Ian Lesnet</text>
<text>Fulfillment by</text>
<text>Bus Pirate</text>
<text>FEB 2018</text>
<text>v3.9</text>
<text>CC-0</text>
<text>Ian Lesnet</text>
<text>Bus Pirate v3.9</text>
<text>FEB 2018</text>
<text>http://dangerousprototypes.com</text>
<text>PGC</text>
<text>PGD</text>
<text>GND</text>
<text>+3V3</text>
<text>!MLCR</text>
<text>GND</text>
<text>3V3</text>
<text>ADC</text>
<text>CS</text>
<text>CLK</text>
<text>MOSI</text>
<text>MISO</text>
<text>AUX</text>
<text>VPU</text>
<text>5V</text>
<text>v.trocio</text>
<text>NC</text>
<text>NC</text>
<text>ICSP</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="SMC_A">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
</packages>
</library>
<library name="wuerth-elektronik">
<packages>
<package name="WE-KI_0805_B">
<description>SMD Wire Wound Ceramic Inductor</description>
</package>
</packages>
</library>
<library name="40xx">
<packages>
<package name="TSSOP14">
<description>&lt;b&gt;plastic thin shrink small outline package; 14 leads; body width 4.4 mm&lt;/b&gt;&lt;p&gt;
SOT402-1&lt;br&gt;
Source: http://www.nxp.com/documents/data_sheet/74ABT125.pdf</description>
</package>
</packages>
</library>
<library name="DP-logo">
<packages>
<package name="DP-LOGO">
</package>
</packages>
</library>
<library name="dp_devices">
<packages>
<package name="R603">
</package>
<package name="C603">
</package>
<package name="RN8P-4R-CRA06S">
</package>
<package name="SSOP28">
<description>SSOP28</description>
</package>
<package name="SOT-23-5">
</package>
<package name="DP_LOGO_ART_1X1">
</package>
<package name="LOGO_CC-0">
</package>
</packages>
</library>
<library name="ohw-logo">
<packages>
<package name="OSHW_8X350_NOTEXT">
</package>
</packages>
</library>
<library name="dp_devices.v6">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="SSOP-16-FTDI">
<description>SSOP-16, 0.32 x 1.26 mm pad, 0.63mm pitch, 6.82mm Pad length</description>
</package>
<package name="DP5050_V1">
</package>
<package name="CON_USB_MICRO-B-1-MD05SMXXX-01">
<description>1-MD05SNXXX-01
&lt;br&gt;Micro USB 5P/F B Type SMT</description>
</package>
<package name="M1X6">
</package>
<package name="M1X10_MALE_RIGHT_ANGLES_PTH_SHROUDED">
<description>Molex PN: 70553-0044
&lt;br&gt; Distance from edge to center: 6.795 mm</description>
</package>
<package name="LED-805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="dp_devices" package="R603" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="dp_devices.v6" package="LED-805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="dp_devices" package="R603" value="1K1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="dp_devices" package="C603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="dp_devices" package="C603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="SMC_A" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="dp_devices.v6" package="LED-805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="dp_devices" package="R603" value="1K1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="dp_devices.v6" package="LED-805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="dp_devices" package="R603" value="1K1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="dp_devices" package="C603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="wuerth-elektronik" package="WE-KI_0805_B" value="700mA+ ferrite">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="SMC_A" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="40xx" package="TSSOP14" value="4066">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="dp_devices" package="C603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3A" library="dp_devices.v6" package="LED-805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2A" library="dp_devices.v6" package="LED-805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1A" library="dp_devices.v6" package="LED-805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="dp_devices" package="R603" value="1K1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="dp_devices" package="C603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="dp_devices" package="C603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="dp_devices" package="C603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="dp_devices" package="C603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="dp_devices" package="C603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="DP-logo" package="DP-LOGO" value=""/>
<element name="LED4" library="dp_devices.v6" package="LED-805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4A" library="dp_devices.v6" package="LED-805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN3" library="dp_devices" package="RN8P-4R-CRA06S" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN1" library="dp_devices" package="RN8P-4R-CRA06S" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN2" library="dp_devices" package="RN8P-4R-CRA06S" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="dp_devices" package="SSOP28" value="PIC24FJ64GA002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR1" library="dp_devices" package="SOT-23-5" value="MCP1801T-3302I/OT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR2" library="dp_devices" package="SOT-23-5" value="MCP1801T-3302I/OT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR3" library="dp_devices" package="SOT-23-5" value="MCP1801T-5002I/OT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="dp_devices" package="DP_LOGO_ART_1X1" value=""/>
<element name="LOGO1" library="dp_devices" package="LOGO_CC-0" value="LOGO_CC-0"/>
<element name="U$2" library="ohw-logo" package="OSHW_8X350_NOTEXT" value=""/>
<element name="IC4" library="dp_devices.v6" package="SSOP-16-FTDI" value="IC_FT230X-SSOP-16">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PCB1" library="dp_devices.v6" package="DP5050_V1" value="PCB_DP_SQUARE-5X5">
<attribute name="PCB_SIZE" value="DP5050_V1"/>
</element>
<element name="RN4" library="dp_devices" package="RN8P-4R-CRA06S" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CON3" library="dp_devices.v6" package="CON_USB_MICRO-B-1-MD05SMXXX-01" value="CON-USB-F-MICRO-B"/>
<element name="CON2" library="dp_devices.v6" package="M1X6" value="CON_HEADER_1X06-PTH">
<attribute name="NAME"/>
</element>
<element name="CON1" library="dp_devices.v6" package="M1X10_MALE_RIGHT_ANGLES_PTH_SHROUDED" value="CON_HEADER_1X10-RIGHT_ANGLED_PTH_SHROUDED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="LED1" pad="C"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C11" pad="-"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="C4" pad="2"/>
<contactref element="C10" pad="-"/>
<contactref element="IC3" pad="7"/>
<contactref element="C3" pad="2"/>
<contactref element="LED3A" pad="C"/>
<contactref element="LED2A" pad="C"/>
<contactref element="LED1A" pad="C"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="RN1" pad="7"/>
<contactref element="RN1" pad="5"/>
<contactref element="RN2" pad="7"/>
<contactref element="RN2" pad="5"/>
<contactref element="IC1" pad="19"/>
<contactref element="IC1" pad="27"/>
<contactref element="IC1" pad="8"/>
<contactref element="VR1" pad="2"/>
<contactref element="VR2" pad="2"/>
<contactref element="VR3" pad="2"/>
<contactref element="IC4" pad="13"/>
<contactref element="IC4" pad="5"/>
<contactref element="RN4" pad="7"/>
<contactref element="RN4" pad="6"/>
<contactref element="RN4" pad="5"/>
<contactref element="CON3" pad="P5"/>
<contactref element="CON3" pad="GND1"/>
<contactref element="CON3" pad="GND6"/>
<contactref element="CON3" pad="GND5"/>
<contactref element="CON3" pad="GND4"/>
<contactref element="CON3" pad="GND3"/>
<contactref element="CON3" pad="GND2"/>
<contactref element="CON2" pad="3"/>
<contactref element="CON1" pad="1"/>
</signal>
<signal name="MCLR">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="CON2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="LED1" pad="A"/>
<contactref element="R2" pad="1"/>
<contactref element="LED1A" pad="A"/>
</signal>
<signal name="PGD">
<contactref element="IC1" pad="4"/>
<contactref element="CON2" pad="4"/>
</signal>
<signal name="PGC">
<contactref element="IC1" pad="5"/>
<contactref element="CON2" pad="5"/>
</signal>
<signal name="TX">
<contactref element="IC1" pad="14"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="RX">
<contactref element="IC1" pad="11"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="C11" pad="+"/>
<contactref element="IC1" pad="20"/>
</signal>
<signal name="VEXTERN">
<contactref element="RN2" pad="8"/>
<contactref element="IC3" pad="2"/>
<contactref element="CON1" pad="4"/>
</signal>
<signal name="ADC1">
<contactref element="RN2" pad="3"/>
<contactref element="RN2" pad="4"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="ADC">
<contactref element="RN2" pad="6"/>
<contactref element="CON1" pad="5"/>
</signal>
<signal name="SWV33">
<contactref element="R6" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="RN1" pad="6"/>
<contactref element="VR2" pad="5"/>
<contactref element="IC3" pad="3"/>
<contactref element="CON1" pad="3"/>
</signal>
<signal name="SWV50">
<contactref element="C9" pad="1"/>
<contactref element="RN1" pad="8"/>
<contactref element="VR3" pad="5"/>
<contactref element="IC3" pad="9"/>
<contactref element="CON1" pad="2"/>
</signal>
<signal name="AUX1">
<contactref element="IC1" pad="21"/>
<contactref element="RN4" pad="1"/>
<contactref element="CON1" pad="6"/>
</signal>
<signal name="ADC2">
<contactref element="RN2" pad="1"/>
<contactref element="RN2" pad="2"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="ADC3">
<contactref element="RN1" pad="3"/>
<contactref element="RN1" pad="4"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="ADC4">
<contactref element="RN1" pad="1"/>
<contactref element="RN1" pad="2"/>
<contactref element="IC1" pad="26"/>
</signal>
<signal name="N$6">
<contactref element="LED2" pad="A"/>
<contactref element="R4" pad="1"/>
<contactref element="LED2A" pad="A"/>
</signal>
<signal name="LD1">
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="VREGEN">
<contactref element="IC1" pad="2"/>
<contactref element="VR2" pad="3"/>
<contactref element="VR3" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="LED3" pad="A"/>
<contactref element="R6" pad="1"/>
<contactref element="LED3A" pad="A"/>
</signal>
<signal name="PULLUPEN">
<contactref element="IC1" pad="22"/>
<contactref element="RN4" pad="2"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="N$15">
<contactref element="IC4" pad="8"/>
<contactref element="CON3" pad="P3"/>
</signal>
<signal name="N$16">
<contactref element="IC4" pad="9"/>
<contactref element="CON3" pad="P2"/>
</signal>
<signal name="$N26">
<contactref element="L1" pad="2"/>
<contactref element="CON3" pad="P1"/>
</signal>
<signal name="RTS">
<contactref element="IC1" pad="12"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="CTS">
<contactref element="IC1" pad="10"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="N$13">
<contactref element="R3" pad="1"/>
<contactref element="LED4" pad="A"/>
<contactref element="LED4A" pad="A"/>
</signal>
<signal name="RXLED">
<contactref element="LED4" pad="C"/>
<contactref element="LED4A" pad="C"/>
<contactref element="IC4" pad="14"/>
</signal>
<signal name="CS">
<contactref element="IC1" pad="15"/>
<contactref element="RN3" pad="7"/>
<contactref element="CON1" pad="7"/>
</signal>
<signal name="CLK">
<contactref element="IC1" pad="17"/>
<contactref element="RN3" pad="5"/>
<contactref element="CON1" pad="9"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="16"/>
<contactref element="RN3" pad="6"/>
<contactref element="CON1" pad="8"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="18"/>
<contactref element="RN3" pad="8"/>
<contactref element="CON1" pad="10"/>
</signal>
<signal name="N$8">
<contactref element="C5" pad="1"/>
<contactref element="IC4" pad="10"/>
</signal>
<signal name="VUSB">
<contactref element="C4" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="C10" pad="+"/>
<contactref element="IC4" pad="12"/>
<contactref element="VR3" pad="1"/>
<contactref element="VR2" pad="1"/>
<contactref element="VR1" pad="1"/>
<contactref element="IC3" pad="14"/>
<contactref element="C3" pad="1"/>
<contactref element="VR1" pad="3"/>
</signal>
<signal name="+3V3">
<contactref element="C7" pad="1"/>
<contactref element="VR1" pad="5"/>
<contactref element="C6" pad="1"/>
<contactref element="IC4" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="28"/>
<contactref element="IC1" pad="13"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="CON2" pad="2"/>
</signal>
<signal name="V33PU">
<contactref element="IC3" pad="5"/>
<contactref element="RN4" pad="3"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="V50PU">
<contactref element="IC3" pad="6"/>
<contactref element="RN4" pad="4"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$10">
<contactref element="IC3" pad="1"/>
<contactref element="RN4" pad="8"/>
<contactref element="RN3" pad="1"/>
<contactref element="RN3" pad="2"/>
<contactref element="RN3" pad="4"/>
<contactref element="RN3" pad="3"/>
<contactref element="IC3" pad="8"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="TP1">
<contactref element="IC1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
